<?xml version="1.0" encoding="utf-8"?>
<JingJiBiao Xmbh="xm001" Xmmc="北京师范大学淮南实验学校西食堂装饰装修及安装工程" Version="1.0" Jsfs="一般计税" Jsdw="1" Zjzmj="0">
  <ZhaoBiaoXx Zbr="1" Zxr="1" ZbrDb="1" ZxrDb="1" Bzr="1" Fhr="1" BzRq="2022-11-18" FhRq="2022-11-18" />
  <Dxgcxx Dxgcmc="北京师范大学淮南实验学校西食堂装饰装修及安装工程" Dxgcbh="dx001" Je="0" Bkjzf="0" Aqwmf="0" Zgj="0" Jzmj="0">
    <Dwgcxx Dwgcbh="00001" Dwgcmc="厨房装饰" Zylb="2" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6DFEC6B44BB3BB8C0B40CBD2DBA20B5E9460A95DCE14113946E3E4F5EC5E8E52420EB3555FB5AA973F" DogNum="97020542FB0B283C" MachineKey="38-F3-AB-49-E2-8E">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="ZF-01" Mc="    环境保护费" Qfjs="0" Fl="1.78" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="ZF-02" Mc="    文明施工费" Qfjs="0" Fl="6.1" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="ZF-03" Mc="    安全施工费" Qfjs="0" Fl="4.22" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="ZF-04" Mc="    临时设施费" Qfjs="0" Fl="4.6" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.1" Bm="ZF-05" Mc="  环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.1" />
  </Bkjzf>
  <Sj>
    <SjMx Xh="1" Mc="税金" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="0111" Mc="楼地面装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="011102003001" Mc="块料楼地面" Xmtz="1、8厚600×600防滑地砖铺实拍平,干水泥擦缝&#xD;&#xA;2、30厚1:3水泥砂浆结合层,表面撒水泥粉地面&#xD;&#xA;3、2.0厚自粘聚合物改性沥青防水卷材(防滑地砖-防水)(无胎)两道 &#xD;&#xA;4、最薄处20厚1:3水泥砂浆找坡，找平&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="941.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="010507003001" Mc="地沟" Xmtz="1、成品排水格栅&#xD;&#xA;2、宽度300mm，深度300mm&#xD;&#xA;3、瓷砖贴面（已计入地面）&#xD;&#xA;4、防水砂浆粉砂层&#xD;&#xA;5、C30防水细石砼地沟，底部40厚，两侧60厚" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m" Sl="120.8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0112" Mc="墙、柱面装饰与隔断、幕墙工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="3" Qdbm="011201001001" Mc="块料墙面" Xmtz="1、素水泥浆一道甩毛(内掺建筑胶)&#xD;&#xA;2、9厚1:3水泥砂浆分层压实抹平&#xD;&#xA;3、2.0厚自粘聚合物改性沥青防水卷材(无胎)两道&#xD;&#xA;4、6厚1:2.5水泥砂浆抹平&#xD;&#xA;5、8厚300×600面砖正背面及四周满涂防污剂(在粘贴面涂专用强力建筑胶后点粘)&#xD;&#xA;6、白水泥擦缝" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1997.8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="011501016001" Mc="窗口" Xmtz="1、12mm阻燃板基层&#xD;&#xA;2、12mm厚钢化玻璃窗口&#xD;&#xA;3、1.5mm铝型材&#xD;&#xA;4、具体做法详见图纸" Gcnr="" Jsgz="1.以个计量，按设计图示数量计量。 &#xD;&#xA;2.以米计量，按设计图示尺寸以延长米计算 &#xD;&#xA;3.以立方米计量，按设计图示尺寸以体积计算。 &#xD;&#xA;2.以米计量，按设计图示尺寸以延长米计算 &#xD;&#xA;3.以立方米计量，按设计图示尺寸以体积计算" Dw="m2" Sl="83.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0113" Mc="天棚工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="5" Qdbm="011302001001" Mc="吊顶天棚" Xmtz="1、吊顶高度：3m&#xD;&#xA;2、结构板,板底预留C10钢筋吊环双向间距1200&#xD;&#xA;3、C8钢筋吊杆,双向间距1200,吊杆上部与吊&#xD;&#xA;4、与安装型式配套的专用上层主龙骨,中距1200,&#xD;&#xA;5、与铝扣板配套的专用下层副龙骨联接,间距600,&#xD;&#xA;6、1.0mm厚铝扣板600X600与配套的专用龙骨固定" Gcnr="" Jsgz="按设计图示尺寸以水平投影面积计算。天棚面中的灯槽及跌级、锯齿形、吊挂式、藻井式天棚面积不展开计算。不扣除间壁墙、检查口、附墙烟囱、柱垛和管道所占面积,扣除单个＞0.3㎡的孔洞、独立柱及与天棚相连的窗帘盒所占的面积。" Dw="m2" Sl="939.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="ZC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="ZC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="ZC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.7" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="ZC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.3" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="ZC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.6" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="ZC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="ZC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="ZC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="8" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
    <Dwgcxx Dwgcbh="00002" Dwgcmc="厨房安装" Zylb="3" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6DFEC6B44BB3BB8C0B40CBD2DBA20B5E9460A95DCE14113946E3E4F5EC5E8E5242ADEA8A27D29294F4" DogNum="97020542FB0B283C" MachineKey="38-F3-AB-49-E2-8E">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="AF-01" Mc="    环境保护费" Qfjs="0" Fl="1.78" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="AF-02" Mc="    文明施工费" Qfjs="0" Fl="6.1" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="AF-03" Mc="    安全施工费" Qfjs="0" Fl="4.22" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="AF-04" Mc="    临时设施费" Qfjs="0" Fl="4.6" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.1" Bm="AF-05" Mc="  环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.1" />
  </Bkjzf>
  <Sj>
    <SjMx Xh="1" Mc="税金" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <Qdmx Xh="1" Qdbm="030404017001" Mc="配电箱" Xmtz="1、名称：AP-CF5&#xD;&#xA;2、规格：详见配电箱系统图&#xD;&#xA;3、安装方式：挂墙安装&#xD;&#xA;4、说明：含接线端子、接线鼻子、含箱内元器件安装&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、焊压接线端子&#xD;&#xA;3、接地" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="2" Qdbm="030404017002" Mc="配电箱" Xmtz="1、名称：AP-CF6&#xD;&#xA;2、规格：详见配电箱系统图&#xD;&#xA;3、安装方式：挂墙安装&#xD;&#xA;4、说明：含接线端子、接线鼻子、含箱内元器件安装&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、焊压接线端子&#xD;&#xA;3、接地" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="3" Qdbm="030404017003" Mc="配电箱" Xmtz="1、名称：AP-CF7&#xD;&#xA;2、规格：详见配电箱系统图&#xD;&#xA;3、安装方式：挂墙安装&#xD;&#xA;4、说明：含接线端子、接线鼻子、含箱内元器件安装&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、焊压接线端子&#xD;&#xA;3、接地" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="4" Qdbm="030404017004" Mc="配电箱" Xmtz="1、名称：AP-CF8&#xD;&#xA;2、规格：详见配电箱系统图&#xD;&#xA;3、安装方式：挂墙安装&#xD;&#xA;4、说明：含接线端子、接线鼻子、含箱内元器件安装&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、焊压接线端子&#xD;&#xA;3、接地" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="5" Qdbm="030404017005" Mc="配电箱" Xmtz="1、名称：控制箱&#xD;&#xA;2、规格：详见配电箱系统图&#xD;&#xA;3、安装方式：挂墙安装&#xD;&#xA;4、说明：含接线端子、接线鼻子、含箱内元器件安装&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、焊压接线端子&#xD;&#xA;3、接地" Jsgz="按设计图示数量计算" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="6" Qdbm="030411003001" Mc="桥架" Xmtz="1、名称：强电桥架&#xD;&#xA;2、型号：300*100&#xD;&#xA;3、包含盖板、连接片、铜带、防雷接地等附件&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、除锈、刷油、防腐" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="11.36" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="7" Qdbm="030411003002" Mc="桥架" Xmtz="1、名称：强电桥架&#xD;&#xA;2、型号：200*100&#xD;&#xA;3、包含盖板、连接片、铜带、防雷接地等附件&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、除锈、刷油、防腐" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="74.91" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="8" Qdbm="030411003003" Mc="桥架" Xmtz="1、名称：强电桥架&#xD;&#xA;2、型号：150*100&#xD;&#xA;3、包含盖板、连接片、铜带、防雷接地等附件&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、除锈、刷油、防腐" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="70.5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="9" Qdbm="030411003004" Mc="桥架" Xmtz="1、名称：强电桥架&#xD;&#xA;2、型号：100*100&#xD;&#xA;3、包含盖板、连接片、铜带、防雷接地等附件&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、除锈、刷油、防腐" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="39.41" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="10" Qdbm="030413001001" Mc="铁构件" Xmtz="1、名称：桥架支撑架&#xD;&#xA;2、包含制作、安装、除锈、刷漆费用。&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装" Jsgz="按设计图示尺寸以质量计算" Dw="t" Sl="0.19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="11" Qdbm="080807013001" Mc="防火堵洞（隔板）、孔洞封堵" Xmtz="1、名称：防火堵洞&#xD;&#xA;2、部位：电气竖井洞口处及竖井桥架内&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="处" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="12" Qdbm="030411001001" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC管&#xD;&#xA;3、规格：DN100&#xD;&#xA;4、配置要求：含配套支架制作及安装等&#xD;&#xA;5、安装形式：暗敷&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="5.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="13" Qdbm="030411001002" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC管&#xD;&#xA;3、规格：DN65&#xD;&#xA;4、配置要求：含配套支架制作及安装等&#xD;&#xA;5、安装形式：暗敷&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="5.9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="14" Qdbm="030411001003" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC管&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、安装形式：暗配&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="18.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="15" Qdbm="030411001004" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC管&#xD;&#xA;3、规格：DN40&#xD;&#xA;4、安装形式：暗配&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="30.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="16" Qdbm="030411001005" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC管&#xD;&#xA;3、规格：DN32&#xD;&#xA;4、安装形式：暗配&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="88.04" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="17" Qdbm="030411001006" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC管&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、安装形式：暗配&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="5.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="18" Qdbm="030411001007" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质、规格：JDG20&#xD;&#xA;3、配置形式及部位：暗配&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="826.7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="19" Qdbm="030411001008" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质、规格：JDG25&#xD;&#xA;3、配置形式及部位：暗配&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="25.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="20" Qdbm="030408001001" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、型号、规格：WDZ-YJY-4X70+1X35&#xD;&#xA;3、敷设方式：沿桥架或配管敷设&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="106.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="21" Qdbm="030408001002" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、型号、规格：WDZ-YJY-4X35+1X16&#xD;&#xA;3、敷设方式：沿桥架或配管敷设&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="26.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="22" Qdbm="030408001003" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、型号、规格：WDZ-YJY-4X25+1X16&#xD;&#xA;3、敷设方式：沿桥架或配管敷设&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="68.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="23" Qdbm="030408001004" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、型号、规格：WDZ-YJY-5X10&#xD;&#xA;3、敷设方式：沿桥架或配管敷设&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="165.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="24" Qdbm="030408001005" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、型号、规格：WDZ-YJY-5X6&#xD;&#xA;3、敷设方式：沿桥架或配管敷设&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="449.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="25" Qdbm="030408001006" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、型号、规格：WDZ-YJY-5x4&#xD;&#xA;3、敷设方式：沿桥架或配管敷设&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="110.1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="26" Qdbm="030408006001" Mc="电力电缆头" Xmtz="1、名称：电力电缆头1KV&#xD;&#xA;2、规格：电缆截面(mm2) ≤10&#xD;&#xA;3、工作内容：制作、安装&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装" Jsgz="按设计图示数量计算" Dw="个" Sl="38" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="27" Qdbm="030408006002" Mc="电力电缆头" Xmtz="1、名称：电力电缆头1KV&#xD;&#xA;2、规格：电缆截面(mm2) ≤35&#xD;&#xA;3、工作内容：制作、安装&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="28" Qdbm="030408006003" Mc="电力电缆头" Xmtz="1、名称：电力电缆头1KV&#xD;&#xA;2、规格：电缆截面(mm2) ≤70&#xD;&#xA;3、工作内容：制作、安装&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="29" Qdbm="030411004001" Mc="配线" Xmtz="1、配线形式：穿管、桥架敷设&#xD;&#xA;2、导线型号、规格、材质：WDZ-BYJ-2.5&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="1737.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="30" Qdbm="030411004002" Mc="配线" Xmtz="1、配线形式：穿管、桥架敷设&#xD;&#xA;2、导线型号、规格、材质：WDZ-BYJ-4&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="1771.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="31" Qdbm="030404034001" Mc="照明开关" Xmtz="1、名称：紫外线消毒灯开关&#xD;&#xA;2、安装方式：壁装&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="32" Qdbm="030404035001" Mc="插座" Xmtz="1、名称：防水防溅插座&#xD;&#xA;2、型号：250V 10A 安全型&#xD;&#xA;3、安装方式：壁装&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="33" Qdbm="030404035002" Mc="插座" Xmtz="1、名称：防水防溅插座&#xD;&#xA;2、型号：250V 16A 安全型&#xD;&#xA;3、安装方式：壁装&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="34" Qdbm="030411006001" Mc="接线盒" Xmtz="1、名称：开关、插座盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、安装形式：暗装&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="35" Qdbm="030411006002" Mc="接线盒" Xmtz="1、名称：接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、安装形式：暗装&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="36" Qdbm="030414002001" Mc="送配电装置系统" Xmtz="1、名称：送配电装置系统&#xD;&#xA;2、电压等级（KV)：1kV 交流供电&#xD;&#xA;3、未尽事宜详见图纸、招标文件、答疑文件、图集、政府相关文件及规范等其他文件" Gcnr="" Jsgz="按设计图示系统计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="37" Qdbm="031001001001" Mc="内衬塑热镀锌钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：DN70&#xD;&#xA;4、连接形式：丝扣连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="10.3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="38" Qdbm="031001001002" Mc="内衬塑热镀锌钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：DN50&#xD;&#xA;4、连接形式：丝扣连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="25.36" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="39" Qdbm="031001001003" Mc="内衬塑热镀锌钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：DN40&#xD;&#xA;4、连接形式：丝扣连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="26.5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="40" Qdbm="031001001004" Mc="内衬塑热镀锌钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：DN32&#xD;&#xA;4、连接形式：丝扣连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="41.77" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="41" Qdbm="031001001005" Mc="内衬塑热镀锌钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：DN25&#xD;&#xA;4、连接形式：丝扣连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="19.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="42" Qdbm="031001001006" Mc="内衬塑热镀锌钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：DN20&#xD;&#xA;4、连接形式：丝扣连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="57.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="43" Qdbm="031001001007" Mc="内衬塑热镀锌钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：DN15&#xD;&#xA;4、连接形式：丝扣连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="275.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="44" Qdbm="WB030817014001" Mc="管道消毒冲洗" Xmtz="1、规格、型号：DN15&#xD;&#xA;2、管内介质：给水&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="275.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="45" Qdbm="WB030817014002" Mc="管道消毒冲洗" Xmtz="1、规格、型号：DN20&#xD;&#xA;2、管内介质：给水&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="57.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="46" Qdbm="WB030817014003" Mc="管道消毒冲洗" Xmtz="1、规格、型号：DN25&#xD;&#xA;2、管内介质：给水&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="19.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="47" Qdbm="WB030817014004" Mc="管道消毒冲洗" Xmtz="1、规格、型号：DN32&#xD;&#xA;2、管内介质：给水&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="41.77" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="48" Qdbm="WB030817014005" Mc="管道消毒冲洗" Xmtz="1、规格、型号：DN40&#xD;&#xA;2、管内介质：给水&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="26.5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="49" Qdbm="WB030817014006" Mc="管道消毒冲洗" Xmtz="1、规格、型号：DN50&#xD;&#xA;2、管内介质：给水&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="25.36" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="50" Qdbm="WB030817014007" Mc="管道消毒冲洗" Xmtz="1、规格、型号：DN65&#xD;&#xA;2、管内介质：给水&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="m" Sl="10.3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="51" Qdbm="031003001001" Mc="螺纹阀门" Xmtz="1、类型：截止阀&#xD;&#xA;2、材质：铜质&#xD;&#xA;3、规格、压力等级：DN15&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="52" Qdbm="031003001002" Mc="螺纹阀门" Xmtz="1、类型：截止阀&#xD;&#xA;2、材质：铜质&#xD;&#xA;3、规格、压力等级：DN32&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="53" Qdbm="031003001003" Mc="螺纹阀门" Xmtz="1、类型：截止阀&#xD;&#xA;2、材质：铜质&#xD;&#xA;3、规格、压力等级：DN40&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="54" Qdbm="031003001004" Mc="螺纹阀门" Xmtz="1、类型：截止阀&#xD;&#xA;2、材质：铜质&#xD;&#xA;3、规格、压力等级：DN70&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="55" Qdbm="031002001001" Mc="管道支吊架制作与安装" Xmtz="1、材质：型钢&#xD;&#xA;2、管架形式：详见设计图纸&#xD;&#xA;3、防腐绝缘：管道支吊架除锈后刷樟丹二道,灰色调和漆二道。但不锈钢管、铜管应在管道与支架间加橡胶垫隔绝。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="456.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="56" Qdbm="031001005001" Mc="柔性接口机制排水铸铁管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：污废水&#xD;&#xA;3、规格、压力等级：DN75&#xD;&#xA;4、连接形式：柔性机械连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、管道管件吊支架、管卡安装及接入室外检查井开孔及封堵等&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="143.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="57" Qdbm="031001005002" Mc="柔性接口机制排水铸铁管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：污废水&#xD;&#xA;3、规格、压力等级：DN100&#xD;&#xA;4、连接形式：柔性机械连接&#xD;&#xA;5、压力试验及吹洗设计要求：详见图纸要求&#xD;&#xA;6、管道管件吊支架、管卡安装及接入室外检查井开孔及封堵等&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="6.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <QdBt Bm="4.1" Mc="清真厨房加工间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="58" Qdbm="ZB030101001001" Mc="四层格栅货架 1200*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="ZB030101001002" Mc="四层格栅货架 1500*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="ZB030101001003" Mc="大单星盆水池 1000*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="031004014001" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="ZB030101001004" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="ZB030101001005" Mc="接手台 500*700*950" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="031004014002" Mc="洗地龙头 10米" Xmtz="1、EPDM软管；&#xD;&#xA;2、敞开式卷盘；&#xD;&#xA;3、带喷头&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="ZB030101001006" Mc="刀具消毒柜 540*135*646" Xmtz="1、优质不锈钢制成，美观耐用；&#xD;&#xA;2、箱内可放置5～10把刀具；&#xD;&#xA;3、设有开门停止紫外线灯工作功能；&#xD;&#xA;4、设有磁性门吸和门锁，锁门功能；&#xD;&#xA;5、设有挂墙孔，可选择悬挂或座台摆放；&#xD;&#xA;6、内置消杀菌功能。&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="ZB030101001007" Mc="双层平板工作台 1800*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="ZB030101001008" Mc="多功能切配台 1800*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="031006012001" Mc="开水器连底座 9KW" Xmtz="1、用料细则：采用优质不锈钢板制作，全自动缺水断电保护装置，微电脑显示，生熟水自动分离环保节能高效。容量：25L；额定功率6KW；供水量80L/H；&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="030412001001" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.2" Mc="清真厨房" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="70" Qdbm="ZB030101001009" Mc="四层格栅货架 1200*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="71" Qdbm="ZB030101001010" Mc="四层格栅货架 1500*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="ZB030101001011" Mc="单星盆水池 700*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="031004014003" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="74" Qdbm="ZB030101001012" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="ZB030101001013" Mc="双层平板工作台 1800*700*800+150" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="ZB030101001014" Mc="风冷四门高身雪柜 单温冷藏" Xmtz="1、配风冷蒸发器；&#xD;&#xA;2、电子式温控器，层架高度可调；&#xD;&#xA;3、高压整体发泡，门框带除露发热丝；&#xD;&#xA;4、R134a或R404a制冷剂；&#xD;&#xA;5、功率：220V/0.75&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="ZB030101001015" Mc="单通工作台 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、趟门轨道，不锈钢滑轮，双向式双移门；   &#xD;&#xA;5、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="031004014004" Mc="洗地龙头 10米" Xmtz="1、EPDM软管；&#xD;&#xA;2、敞开式卷盘；&#xD;&#xA;3、带喷头&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="031006012002" Mc="开水器连底座 9KW" Xmtz="1、用料细则：采用优质不锈钢板制作，全自动缺水断电保护装置，微电脑显示，生熟水自动分离环保节能高效。容量：25L；额定功率6KW；供水量80L/H；&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="ZB030101001016" Mc="单通工作台 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、趟门轨道，不锈钢滑轮，双向式双移门；   &#xD;&#xA;5、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="81" Qdbm="ZB030101001017" Mc="双星水池（背靠式）1460*700*800" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="ZB030101001018" Mc="双门平台雪柜 1800*760*800" Xmtz="1、配风冷蒸发器；&#xD;&#xA;2、电子式温控器，层架高度可调；&#xD;&#xA;3、高压整体发泡，门框带除露发热丝；&#xD;&#xA;4、R134a或R404a制冷剂；&#xD;&#xA;5、功率：220V/0.76&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="83" Qdbm="ZB030101001019" Mc="三层台面立架 1800*350*900" Xmtz="1、采用SUS304不锈钢板焊接而成；&#xD;&#xA;2、主板、层板采用1.5mm 不锈钢板制作；&#xD;&#xA;3、下加不不锈钢加强筋；&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="ZB030101001020" Mc="炉拼台 400*1200*1200" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、立管：Φ38*1.0mm不锈钢圆管；&#xD;&#xA;3、横档：38*25*1.2mm不锈钢矩管；&#xD;&#xA;4、脚:不锈钢可调子弹脚。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="ZB030101001021" Mc="燃气单头大锅灶 1100*1200*1200" Xmtz="1、台面：1.5mm优质304不锈钢板、带冷却水；&#xD;&#xA;2、侧板、背板：1.0mm 304不锈钢板；&#xD;&#xA;3、炉脚：Φ直径50mm钢管,外包不锈钢套管；&#xD;&#xA;4、节能静音预混式炉头，带电子点火，熄火保护。&#xD;&#xA;5、需达到一级能效&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="86" Qdbm="ZB030101001022" Mc="双头双尾炒灶 2000*1200*1200" Xmtz="1、台面：1.5mm优质304不锈钢板、带冷却水；&#xD;&#xA;2、侧板、背板：1.0mm 304不锈钢板；&#xD;&#xA;3、炉脚：Φ直径51mm钢管,外包不锈钢套管；&#xD;&#xA;4、节能静音预混式炉头，带电子点火，熄火保护。&#xD;&#xA;5、需达到一级能效&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="ZB030101001023" Mc="六眼煲仔炉 1000*1200*1200" Xmtz="1、台面,1.5mm优质304不锈钢雪花拉丝板；&#xD;&#xA;2、侧板、背板：1.0mm 优质304不锈钢雪花拉丝板；&#xD;&#xA;3、炉脚：Φ38mm*1.0mm不锈钢脚，配电子点火，熄火保护。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="88" Qdbm="ZB030101001024" Mc="燃气双头矮汤炉 1300*700*500+700" Xmtz="1、台面,1.5mm优质304不锈钢雪花拉丝板；&#xD;&#xA;2、侧板、背板：1.0mm 优质304不锈钢雪花拉丝板；&#xD;&#xA;3、炉脚：Φ38mm*1.5mm不锈钢脚；&#xD;&#xA;4、带熄火保护。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="89" Qdbm="ZB030101001025" Mc="烤箱 双门" Xmtz="1、全不锈钢面板结构,永不生锈,坚固耐用；&#xD;&#xA;2、全密封式整体耐高温材料保温结构,保温性能好,加热时间短；&#xD;&#xA;3、特设300℃超高温自复位断路保护器,为您的机器披上一件高温底线防护外衣；&#xD;&#xA;4、精密准确的定时控制装置,烘烤更轻松自如；&#xD;&#xA;5、炉面、炉底温度双重控制；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="030703017001" Mc="不锈钢油网烟罩 7900*1300*500" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm，加强筋1.2mm；&#xD;&#xA;3、配不锈钢滴油杯及LED光源；&#xD;&#xA;4、配滴油杯。&#xD;&#xA;5、带岗位补风系统；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="91" Qdbm="030703017002" Mc="L型烟罩上封板（含支架及上下导槽） L=7900" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="030703017003" Mc="不锈钢落地式封墙板 L=7900" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="ZB030101001026" Mc="烟罩自动灭火系统" Xmtz="1、全不锈钢面板结构,永不生锈,坚固耐用；&#xD;&#xA;2、全密封式整体耐高温材料保温结构,保温性能好,加热时间短；&#xD;&#xA;3、灭火药剂为食用油专用灭火药剂，该药剂应无毒、无污染、易清洗&#xD;&#xA;4、具有水冷却功能的装置，在灭火剂完全喷射后，水流联动阀立即启动；&#xD;&#xA;5、灭火系统具有自动启动、手动启动、机械启动功能，且不会复燃，能提供消防中控信号及燃气切断功能信号。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="030412001002" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.3" Mc="烹饪间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="95" Qdbm="ZB030101001027" Mc="风冷四门高身雪柜 单温冷藏" Xmtz="1、配风冷蒸发器；&#xD;&#xA;2、电子式温控器，层架高度可调；&#xD;&#xA;3、高压整体发泡，门框带除露发热丝；&#xD;&#xA;4、R134a或R404a制冷剂；&#xD;&#xA;5、功率：220V/0.75&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="ZB030101001028" Mc="风冷六门高身雪柜 单温冷藏" Xmtz="1、配风冷蒸发器；&#xD;&#xA;2、电子式温控器，层架高度可调；&#xD;&#xA;3、高压整体发泡，门框带除露发热丝；&#xD;&#xA;4、R134a或R404a制冷剂；&#xD;&#xA;5、功率：220V/0.75&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="ZB030101001029" Mc="单星盆水池 700*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="98" Qdbm="031004014005" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="99" Qdbm="ZB030101001030" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="031004014006" Mc="洗地龙头 10米" Xmtz="1、EPDM软管；&#xD;&#xA;2、敞开式卷盘；&#xD;&#xA;3、带喷头&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="ZB030101001031" Mc="刀具菜墩消毒柜 1380*680*1800" Xmtz="1、采用优质油磨304不锈钢冷轧板制造；&#xD;&#xA;2、柜体承重采用1.2mm，加强筋1.2mm；&#xD;&#xA;3、消毒方式：热风循环；&#xD;&#xA;4、储存空间：双门単室；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="102" Qdbm="ZB030101001032" Mc="四层格栅货架 1200*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="ZB030101001033" Mc="四层格栅货架 1460*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="ZB030101001034" Mc="保鲜工作台 1800*800*800" Xmtz="1、精制无磁全钢管，钢制蒸发管，整体发泡搁物架采用钢丝浸塑工艺制造J磁吸式自回旋门。&#xD;&#xA;2、配合资压缩机组和温控机&#xD;&#xA;3、参数195W/220V温度范围0至10摄氏度环戊烷聚氨酯整体模具发泡，自动发泡设备、工艺稳定、无氟环保&#xD;&#xA;4、不锈钢门衬板和内底板均采用模具整体拉伸成型，内底板为圆弧拐角，易清洗，满足卫生标准&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="ZB030101001035" Mc="单通工作台 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、趟门轨道，不锈钢滑轮，双向式双移门；   &#xD;&#xA;5、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="ZB030101001036" Mc="三层台面立架 1800*350*900" Xmtz="1、采用SUS304不锈钢板焊接而成；&#xD;&#xA;2、主板、层板采用1.5mm 不锈钢板制作；&#xD;&#xA;3、下加不不锈钢加强筋；&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="ZB030101001037" Mc="双星水池（背靠式）1460*700*800" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="108" Qdbm="ZB030101001038" Mc="炉拼台 400*1100*1200" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、立管：Φ38*1.0mm不锈钢圆管；&#xD;&#xA;3、横档：38*25*1.2mm不锈钢矩管；&#xD;&#xA;4、脚:不锈钢可调子弹脚。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="109" Qdbm="ZB030101001039" Mc="双头双尾炒灶 2000*1100*1200" Xmtz="1、台面：1.5mm优质304不锈钢板、带冷却水；&#xD;&#xA;2、侧板、背板：1.0mm 304不锈钢板；&#xD;&#xA;3、炉脚：Φ直径51mm钢管,外包不锈钢套管；&#xD;&#xA;4、节能静音预混式炉头，带电子点火，熄火保护。&#xD;&#xA;5、需达到一级能效&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="110" Qdbm="ZB030101001040" Mc="燃气单头大锅灶 1100*1100*1200" Xmtz="1、台面：1.5mm优质304不锈钢板、带冷却水；&#xD;&#xA;2、侧板、背板：1.0mm 304不锈钢板；&#xD;&#xA;3、炉脚：Φ直径50mm钢管,外包不锈钢套管；&#xD;&#xA;4、节能静音预混式炉头，带电子点火，熄火保护。&#xD;&#xA;5、需达到一级能效&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="111" Qdbm="ZB030101001041" Mc="燃气双头大锅灶 2000*1100*1200" Xmtz="1、台面：1.5mm优质304不锈钢板、带冷却水；&#xD;&#xA;2、侧板、背板：1.0mm 304不锈钢板；&#xD;&#xA;3、炉脚：Φ直径50mm钢管,外包不锈钢套管；&#xD;&#xA;4、节能静音预混式炉头，带电子点火，熄火保护。&#xD;&#xA;5、需达到一级能效&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="112" Qdbm="030703017004" Mc="不锈钢油网烟罩 13900*1300*500" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm，加强筋1.2mm；&#xD;&#xA;3、配不锈钢滴油杯及LED光源；&#xD;&#xA;4、配滴油杯。&#xD;&#xA;5、带岗位补风系统；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="113" Qdbm="030703017005" Mc="L型烟罩上封板（含支架及上下导槽） L=15200" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="114" Qdbm="030703017006" Mc="不锈钢落地式封墙板 L=13900" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="115" Qdbm="ZB030101001042" Mc="烟罩自动灭火系统 双瓶组" Xmtz="1、全不锈钢面板结构,永不生锈,坚固耐用；&#xD;&#xA;2、全密封式整体耐高温材料保温结构,保温性能好,加热时间短；&#xD;&#xA;3、灭火药剂为食用油专用灭火药剂，该药剂应无毒、无污染、易清洗&#xD;&#xA;4、具有水冷却功能的装置，在灭火剂完全喷射后，水流联动阀立即启动；&#xD;&#xA;5、灭火系统具有自动启动、手动启动、机械启动功能，且不会复燃，能提供消防中控信号及燃气切断功能信号。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="116" Qdbm="030412001003" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.4" Mc="蒸煮间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="117" Qdbm="ZB030101001043" Mc="四层格栅货架 1200*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="118" Qdbm="ZB030101001044" Mc="四层格栅货架 1500*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="119" Qdbm="ZB030101001045" Mc="燃气摇摆汤锅 200L" Xmtz="1、优质304不锈钢制造；&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="120" Qdbm="ZB030101001046" Mc="燃气双门蒸饭车 24盘" Xmtz="1、优质304不锈钢冷轧板制造；&#xD;&#xA;2、面板1.5mm，内胆1.2mm，加强筋1.5mm&#xD;&#xA;3、水箱采用5.0mm钢板，发热仓为钢管；&#xD;&#xA;4、内置蒸汽机；&#xD;&#xA;5、缺水断电保护、意外熄火保护、过压安全保护；&#xD;&#xA;6、需达到一级能效；&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="121" Qdbm="ZB030101001047" Mc="洗米机" Xmtz="1、名称：洗米机&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="122" Qdbm="ZB030101001048" Mc="大单星盆水池 1000*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="123" Qdbm="031004014007" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="124" Qdbm="ZB030101001049" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="125" Qdbm="ZB030101001050" Mc="饼盘车 465*630*1690" Xmtz="1、优质304不锈钢板材制作；&#xD;&#xA;2、厚度1.2mm,配万向轮。&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="126" Qdbm="WB030701004001" Mc="油烟净化一体机 2200*1300*700" Xmtz="1、选用不锈钢板，采用厚度 1.2mm 不锈钢板加工；&#xD;&#xA;2、下端设有接油槽、接油盒，每套排烟罩配防爆灯及吊装接&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="127" Qdbm="030703017007" Mc="L型烟罩上封板（含支架及上下导槽） L=5600" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="128" Qdbm="030703017008" Mc="不锈钢落地式封墙板 L=4300" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="129" Qdbm="030703017009" Mc="不锈钢油网烟罩 6500*1300*500" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm，加强筋1.2mm；&#xD;&#xA;3、配不锈钢滴油杯及LED光源；&#xD;&#xA;4、配滴油杯。&#xD;&#xA;5、带岗位补风系统；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="130" Qdbm="030703017010" Mc="L型烟罩上封板（含支架及上下导槽） L=6500" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="131" Qdbm="030703017011" Mc="不锈钢落地式封墙板 L=6500" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="132" Qdbm="030412001004" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.5" Mc="备餐间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="133" Qdbm="ZB030101001051" Mc="单门宴会保温车 单门" Xmtz="1、减少食物的水分流失&#xD;&#xA;2、保持湿度&#xD;&#xA;3、保证食物原有的口感&#xD;&#xA;4、延长食物保存时间&#xD;&#xA;5、低能耗、无需排风系统&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="134" Qdbm="ZB030101001052" Mc="备餐柜连水吧 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="135" Qdbm="031006012003" Mc="开水器 6KW" Xmtz="1、用料细则：采用优质不锈钢板制作，全自动缺水断电保护装置，微电脑显示，生熟水自动分离环保节能高效。容量：25L；额定功率6KW；供水量80L/H；&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="136" Qdbm="ZB030101001053" Mc="单通工作台 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、趟门轨道，不锈钢滑轮，双向式双移门；   &#xD;&#xA;5、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="137" Qdbm="030412001005" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="138" Qdbm="030412001006" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.6" Mc="面食加工间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="139" Qdbm="ZB030101001054" Mc="卧式和面机 50型KG/945*570*1015" Xmtz="1、规格：50KG  945*570*1015&#xD;&#xA;2、技术要求：整体采用全封闭不锈钢机身，美观卫生&#xD;&#xA;3、采用减速机传动，高效静音  传动机需注油防止漏面黑面&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="140" Qdbm="ZB030101001055" Mc="压面机" Xmtz="1、额定电压:3~380V；&#xD;&#xA;2、电机功率:1.5kW；&#xD;&#xA;3、压面厚度:2~32mm；&#xD;&#xA;4、压面宽度:320mm；&#xD;&#xA;5、外形尺寸:720x830x110mm&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="141" Qdbm="ZB030101001056" Mc="搅拌机" Xmtz="1、料桶容积 : 30L；&#xD;&#xA;2、额定电压 : ~220V/ ~380V；&#xD;&#xA;3、额定频率 : 50Hz；&#xD;&#xA;4、电机功率 : 1.50kW；&#xD;&#xA;5、最大和面量 : 30kg；&#xD;&#xA;6、搅拌转速 : 91/164/294(r/min)&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="142" Qdbm="ZB030101001057" Mc="双星水池 1200*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="143" Qdbm="031004014008" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="144" Qdbm="ZB030101001058" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="145" Qdbm="ZB030101001059" Mc="饼盘车 465*630*1690" Xmtz="1、优质304不锈钢板材制作；&#xD;&#xA;2、厚度1.2mm,配万向轮。&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="146" Qdbm="ZB030101001060" Mc="风冷四门高身雪柜 单温冷藏" Xmtz="1、配风冷蒸发器；&#xD;&#xA;2、电子式温控器，层架高度可调；&#xD;&#xA;3、高压整体发泡，门框带除露发热丝；&#xD;&#xA;4、R134a或R404a制冷剂；&#xD;&#xA;5、功率：220V/0.75&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="147" Qdbm="ZB030101001061" Mc="单通工作台 1600*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、趟门轨道，不锈钢滑轮，双向式双移门；   &#xD;&#xA;5、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="148" Qdbm="ZB030101001062" Mc="木案工作台 1800*800*800" Xmtz="1、台面：优质柳案木；&#xD;&#xA;2、排挡、加强筋：1.5mm不锈钢板；&#xD;&#xA;3、立管：Φ38*1.0mm不锈钢圆管；&#xD;&#xA;4、脚:不锈钢可调子弹脚。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="149" Qdbm="ZB030101001063" Mc="电饼铛" Xmtz="1、外形尺寸：720*600*780；&#xD;&#xA;2、全面采用304不锈钢制造；&#xD;&#xA;3、箱盖采购不锈钢拉伸成型；&#xD;&#xA;4、设备功率：380v/5kw。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="150" Qdbm="ZB030101001064" Mc="接手台 500*700*950" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="151" Qdbm="ZB030101001065" Mc="油炸锅 立式" Xmtz="1、﹣温度范围：0~200℃；&#xD;&#xA;2、﹣380V/9kw。&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="152" Qdbm="ZB030101001066" Mc="醒发箱" Xmtz="1、外表面板材：不锈钢板材无PU保温层&#xD;&#xA;2、控制模式：机械控制面板&#xD;&#xA;3、整个醒发箱上下的温度与湿度很均匀&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="153" Qdbm="ZB030101001067" Mc="烤箱" Xmtz="1、功率/电压：20KW/380V；&#xD;&#xA;2、尺寸 : 1240x860x1515mm    &#xD;&#xA;3、烤箱温度：0-380℃&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="154" Qdbm="030703017012" Mc="不锈钢油网烟罩 5500*1300*500" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm，加强筋1.2mm；&#xD;&#xA;3、配不锈钢滴油杯及LED光源；&#xD;&#xA;4、配滴油杯。&#xD;&#xA;5、带岗位补风系统；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="155" Qdbm="030703017013" Mc="L型烟罩上封板（含支架及上下导槽） L=6800" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="156" Qdbm="030703017014" Mc="不锈钢落地式封墙板 L=5500" Xmtz="1、优质SUS304不锈钢制造；&#xD;&#xA;2、壳体面板1.2mm;&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="157" Qdbm="030412001007" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="158" Qdbm="030412001008" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.7" Mc="预进间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="159" Qdbm="ZB030101001068" Mc="洗手池 500*400*300" Xmtz="1、采用优质SUS304不锈钢板材制作；&#xD;&#xA;2、台面厚1.5mm；加强处理；&#xD;&#xA;3、盆池1.2mm厚不锈钢板制作；&#xD;&#xA;4、配优质不锈钢漏水网&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="160" Qdbm="031004014009" Mc="感应龙头" Xmtz="1、单孔感应龙头&#xD;&#xA;2、台式安装，铸造水嘴；&#xD;&#xA;3、AC-DC控制模块。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="161" Qdbm="030412001009" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="162" Qdbm="030412001010" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.8" Mc="售卖窗口" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="163" Qdbm="ZB030101001069" Mc="五格保温售饭柜 1800*700*800" Xmtz="1、采用优质不锈钢冷轧板制造；&#xD;&#xA;2、台面1.5mm，背板1.2mm；&#xD;&#xA;3、内置保温加热内胆；   &#xD;&#xA;4、通脚锥形不锈钢圆管，配调节脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="164" Qdbm="ZB030101001070" Mc="暖饭车 600*600*800" Xmtz="1、采用优质SUS304不锈钢冷轧板制造；&#xD;&#xA;2、台面1.5mm，背板1.3mm；&#xD;&#xA;3、内置保温加热内胆；   &#xD;&#xA;4、配4吋静音脚轮；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="165" Qdbm="ZB030101001071" Mc="工作台 800*700*950" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="166" Qdbm="ZB030101001072" Mc="工作台 900*700*950" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="167" Qdbm="ZB030101001073" Mc="单星盆水池 700*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="168" Qdbm="031004014010" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="169" Qdbm="ZB030101001074" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="170" Qdbm="ZB030101001075" Mc="单通工作台 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、趟门轨道，不锈钢滑轮，双向式双移门；   &#xD;&#xA;5、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="171" Qdbm="ZB030101001076" Mc="双门不锈钢门消毒柜 双门" Xmtz="1、采用优质油磨304不锈钢冷轧板制造；&#xD;&#xA;2、柜体承重采用1.5mm，加强筋1.2mm；&#xD;&#xA;3、消毒方式：高温热风循环；&#xD;&#xA;4、储存空间：双门単室；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="172" Qdbm="ZB030101001077" Mc="食品留样柜 单温冷藏" Xmtz="1、配风冷蒸发器；&#xD;&#xA;2、电子式温控器，层架高度可调；&#xD;&#xA;3、高压整体发泡，门框带除露发热丝；&#xD;&#xA;4、R134a或R404a制冷剂；&#xD;&#xA;5、功率：220V/0.75&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="173" Qdbm="030412001011" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="174" Qdbm="030412001012" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.9" Mc="清真特色区" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="175" Qdbm="ZB030101001078" Mc="五格保温售饭柜 1800*700*800" Xmtz="1、采用优质不锈钢冷轧板制造；&#xD;&#xA;2、台面1.5mm，背板1.2mm；&#xD;&#xA;3、内置保温加热内胆；   &#xD;&#xA;4、通脚锥形不锈钢圆管，配调节脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="176" Qdbm="ZB030101001079" Mc="暖饭车 600*600*800" Xmtz="1、采用优质SUS304不锈钢冷轧板制造；&#xD;&#xA;2、台面1.5mm，背板1.3mm；&#xD;&#xA;3、内置保温加热内胆；   &#xD;&#xA;4、配4吋静音脚轮；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="177" Qdbm="ZB030101001080" Mc="工作台 1500*700*950" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="178" Qdbm="ZB030101001081" Mc="掩门柜 500*700*850+70" Xmtz="1、优质一级不锈钢制作；&#xD;&#xA;2、台面 SUS304 /1.5mm，对开门SUS304/1.2mm；&#xD;&#xA;3、层板、底板 SUS304/1.2mm；&#xD;&#xA;4、侧板、背板 1.2mm，加强筋 1.5mm；&#xD;&#xA;5、配不锈钢锥形重力脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="179" Qdbm="ZB030101001082" Mc="扒炉连下柜 700*700*850+70" Xmtz="1、优质SUS304/1.5不锈钢制造；&#xD;&#xA;2、功率:380V/7.4KW&#xD;&#xA;3、扒板周围凹槽设计，易清洁；&#xD;&#xA;4、配不锈钢重型调节脚；&#xD;&#xA;5、范围（60℃-200℃）精确控温&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="180" Qdbm="ZB030101001083" Mc="煮面炉 700*700*850+70" Xmtz="1、优质SUS304/1.5不锈钢制造；&#xD;&#xA;2、380V/9KW*2&#xD;&#xA;3、防干烧保护，水位溢出保护；&#xD;&#xA;4、配12φ120mm*H135mm面斗；&#xD;&#xA;5、范围（60℃-200℃）精确控温&#xD;&#xA;6、规格（mm）：700*750*850+50&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="181" Qdbm="ZB030101001084" Mc="汤匙柜 700*700*850+70" Xmtz="1、优质SUS304/1.5不锈钢制造；&#xD;&#xA;2、380V/9KW*2&#xD;&#xA;3、防干烧保护，水位溢出保护；&#xD;&#xA;4、配12φ120mm*H135mm面斗；&#xD;&#xA;5、范围（60℃-200℃）精确控温&#xD;&#xA;6、规格（mm）：700*750*850+51&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="182" Qdbm="030412001013" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="183" Qdbm="030412001014" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.10" Mc="餐具存放处" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="184" Qdbm="ZB030101001085" Mc="高身储物柜 1200*500*1800" Xmtz="1、采用优质1.5mmSUS304不锈钢制作；&#xD;&#xA;2、面板、侧板、门板、底板标厚为1.5mm；&#xD;&#xA;3、后背、层板标厚为1.5mm；&#xD;&#xA;4、全不锈钢锥形脚，加强梁全部不锈钢；&#xD;&#xA;5、门下置塑料滑轮。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="185" Qdbm="030412001015" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.11" Mc="备餐" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="186" Qdbm="ZB030101001086" Mc="备餐柜 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="187" Qdbm="031006012004" Mc="开水器 6KW" Xmtz="1、用料细则：采用优质不锈钢板制作，全自动缺水断电保护装置，微电脑显示，生熟水自动分离环保节能高效。容量：25L；额定功率6KW；供水量80L/H；&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="188" Qdbm="ZB030101001087" Mc="单通工作台 1800*700*800" Xmtz="1、采用优质304不锈钢制造，台面1.5㎜不锈钢制造&#xD;&#xA;2、内置层板采用1.2㎜不锈钢制造；&#xD;&#xA;3、门1.0mm，侧板1.0mm；&#xD;&#xA;4、趟门轨道，不锈钢滑轮，双向式双移门；   &#xD;&#xA;5、通脚锥形不锈钢圆管，配调节脚。&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="189" Qdbm="030412001016" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="190" Qdbm="030412001017" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.12" Mc="肉类加工间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="191" Qdbm="ZB030101001088" Mc="杀鱼台 1500*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.2mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="192" Qdbm="ZB030101001089" Mc="大单星盆水池 1000*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="193" Qdbm="031004014011" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="194" Qdbm="ZB030101001090" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="195" Qdbm="ZB030101001091" Mc="接手台 500*700*950" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="196" Qdbm="ZB030101001092" Mc="刀具消毒柜 540*135*646" Xmtz="1、优质不锈钢制成，美观耐用；&#xD;&#xA;2、箱内可放置5～10把刀具；&#xD;&#xA;3、设有开门停止紫外线灯工作功能；&#xD;&#xA;4、设有磁性门吸和门锁，锁门功能；&#xD;&#xA;5、设有挂墙孔，可选择悬挂或座台摆放；&#xD;&#xA;6、内置消杀菌功能。&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="197" Qdbm="031006012005" Mc="开水器连底座 9KW" Xmtz="1、用料细则：采用优质不锈钢板制作，全自动缺水断电保护装置，微电脑显示，生熟水自动分离环保节能高效。容量：25L；额定功率6KW；供水量80L/H；&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="198" Qdbm="031004014012" Mc="洗地龙头 10米" Xmtz="1、EPDM软管；&#xD;&#xA;2、敞开式卷盘；&#xD;&#xA;3、带喷头&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="199" Qdbm="ZB030101001093" Mc="双层平板工作台 1800*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="200" Qdbm="ZB030101001094" Mc="多功能切配台 1800*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="201" Qdbm="ZB030101001095" Mc="双层平板工作台 1600*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="202" Qdbm="ZB030101001096" Mc="绞切机" Xmtz="1、功率：220V/2.2KW；&#xD;&#xA;2、加工能力：切片400/切丝300/绞肉150；&#xD;&#xA;3、转速：1400；&#xD;&#xA;4、设备重量：73KG；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="203" Qdbm="ZB030101001097" Mc="四层格栅货架 1200*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="204" Qdbm="030412001018" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="205" Qdbm="030412001019" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.13" Mc="蔬菜加工间" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="206" Qdbm="ZB030101001098" Mc="大单星盆水池 1000*700*950" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.0mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="207" Qdbm="031004014013" Mc="水龙头" Xmtz="1、名称：水龙头&#xD;&#xA;2、台式龙头间距4寸，摆动式水嘴；&#xD;&#xA;3、金属陶瓷阀芯，一字型手柄; &#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="208" Qdbm="ZB030101001099" Mc="去水制" Xmtz="1、弯杆排水阀、排水接头；&#xD;&#xA;2、采用标准的 2寸出水接头；&#xD;&#xA;3、安装于3寸水槽开孔，带排水阀。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="209" Qdbm="ZB030101001100" Mc="接手台 500*700*950" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="210" Qdbm="ZB030101001101" Mc="刀具消毒柜 540*135*646" Xmtz="1、优质不锈钢制成，美观耐用；&#xD;&#xA;2、箱内可放置5～10把刀具；&#xD;&#xA;3、设有开门停止紫外线灯工作功能；&#xD;&#xA;4、设有磁性门吸和门锁，锁门功能；&#xD;&#xA;5、设有挂墙孔，可选择悬挂或座台摆放；&#xD;&#xA;6、内置消杀菌功能。&#xD;&#xA;7、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="211" Qdbm="031004014014" Mc="洗地龙头 10米" Xmtz="1、EPDM软管；&#xD;&#xA;2、敞开式卷盘；&#xD;&#xA;3、带喷头&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="212" Qdbm="ZB030101001102" Mc="双层平板工作台 1800*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="213" Qdbm="ZB030101001103" Mc="多功能切配台 1800*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="214" Qdbm="ZB030101001104" Mc="双层平板工作台 1600*800*800" Xmtz="1、台面：1.5mm优质304不锈钢板；&#xD;&#xA;2、层板：1.2mm优质304不锈钢板；&#xD;&#xA;3、加强筋：1.2mm优质304不锈钢板&#xD;&#xA;4、立管：Φ38*1.2mm不锈钢圆管；&#xD;&#xA;5、脚:不锈钢可调子弹脚；&#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="215" Qdbm="ZB030101001105" Mc="土豆去皮机" Xmtz="1、外形尺寸：850*830*800；&#xD;&#xA;2、料筒容积：30kg；&#xD;&#xA;3、功率：1.5kw/380v&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="216" Qdbm="ZB030101001106" Mc="多功能切菜机" Xmtz="1、产量：800-1000KG/H；&#xD;&#xA;2、适用范围：将根茎类（如：马铃薯、蕃薯、芋头、瓜类、洋葱、茄子等）切成丁、片、丝、条状；叶菜类（如：芹菜、大白菜、高丽菜、菠菜、葱等）的长条状之物切成片、丝、段；&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="217" Qdbm="ZB030101001107" Mc="四层格栅货架 1200*500*1550" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="218" Qdbm="030412001020" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="219" Qdbm="030412001021" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.14" Mc="高温冷库" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="220" Qdbm="ZB030101001108" Mc="冷藏库 3400*4300*2600" Xmtz="1、库板选用双面不锈钢板构成的硬质聚氨酯隔热夹芯板，厚度100mm,密度38~40kg/m³，高压发泡工艺一次灌注成型；&#xD;&#xA;2、优质全封闭风冷式制冷机组，具有能耗低、高制冷、能力强、噪音低等特点。&#xD;&#xA;3、冷凝散热器配用高效风冷装置，冷凝器选用外转子低噪音电机，能有效散发热量；&#xD;&#xA;4、库温：冷藏库库温0~5℃，制冷机组选用国内知名一线品牌。配重力回归门。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="221" Qdbm="ZB030101001109" Mc="四层格栅货架 1200*500*1600" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.15" Mc="低温冷库" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="222" Qdbm="ZB030101001110" Mc="冷冻库 3400*4800*2600" Xmtz="1、库板选用双面不锈钢板构成的硬质聚氨酯隔热夹芯板，厚度100mm,密度38~40kg/m³，高压发泡工艺一次灌注成型；&#xD;&#xA;2、优质全封闭风冷式制冷机组，具有能耗低、高制冷、能力强、噪音低等特点。&#xD;&#xA;3、冷凝散热器配用高效风冷装置，冷凝器选用外转子低噪音电机，能有效散发热量；&#xD;&#xA;4、库温：冷藏库库温-18℃~-22℃，制冷机组选用国内知名一线品牌。配重力回归门。&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="223" Qdbm="ZB030101001111" Mc="四层格栅货架 1200*500*1600" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.16" Mc="副食库" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="224" Qdbm="ZB030101001112" Mc="四层格栅货架 1200*500*1600" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="225" Qdbm="ZB030101001113" Mc="四层平板货架 1200*500*1600" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="226" Qdbm="ZB030101001114" Mc="四层格栅货架 1500*500*1600" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="227" Qdbm="ZB030101001115" Mc="平板推车 900*500*900" Xmtz="1、采用优质油磨304不锈钢冷轧板制造&#xD;&#xA;2、格挡1.0mm，加强筋1.2mm&#xD;&#xA;3、配4寸静音耐磨脚轮&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="228" Qdbm="030412001022" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.17" Mc="主食库" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="229" Qdbm="ZB030101001116" Mc="大米架 1200*500*300" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="230" Qdbm="ZB030101001117" Mc="四层平板货架 1200*500*1600" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="231" Qdbm="ZB030101001118" Mc="平板推车 900*500*900" Xmtz="1、采用优质油磨304不锈钢冷轧板制造&#xD;&#xA;2、格挡1.0mm，加强筋1.2mm&#xD;&#xA;3、配4寸静音耐磨脚轮&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="232" Qdbm="030412001023" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.18" Mc="过道" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="233" Qdbm="030412001024" Mc="灭蝇灯" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：50平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.19" Mc="收碗区" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="234" Qdbm="ZB030101001119" Mc="餐厨垃圾回收柜 800*760*800" Xmtz="1、台面：1.5mm优质SUS304不锈钢板；&#xD;&#xA;2、加强筋：1.5mm不锈钢板；&#xD;&#xA;3、立管：Φ38*1.5mm不锈钢圆管；&#xD;&#xA;4、脚:不锈钢可调子弹脚&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="235" Qdbm="ZB030101001120" Mc="碗碟回收 1500*760*800" Xmtz="1、台面：1.5mm优质SUS304不锈钢板；&#xD;&#xA;2、加强筋：1.5mm不锈钢板；&#xD;&#xA;3、立管：Φ38*1.5mm不锈钢圆管；&#xD;&#xA;4、脚:不锈钢可调子弹脚&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="236" Qdbm="031004014015" Mc="洗地龙头 10米" Xmtz="1、EPDM软管；&#xD;&#xA;2、敞开式卷盘；&#xD;&#xA;3、带喷头&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="237" Qdbm="ZB030101001121" Mc="长龙洗碗机" Xmtz="1、全自动传送餐具，对碗碟等餐具进行清洗、漂洗和烘干；&#xD;&#xA;2、最大耗水量320升/小时；   &#xD;&#xA;3、总功率小于等于70kW；&#xD;&#xA;4、清洗数量：最大3000件（6寸碟/小时）；&#xD;&#xA;5、进水电磁阀自带过滤网。独立的漂洗电机、漂洗水箱，保证漂洗水温始终恒定； &#xD;&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="238" Qdbm="ZB030101001122" Mc="大单星浸泡池 1500*800*800" Xmtz="1、台面：SUS304，1.5mm优质不锈钢板；&#xD;&#xA;2、星盆：SUS304，1.2mm优质不锈钢板；&#xD;&#xA;3、加强筋、管脚：Φ38mm*1.2mm不锈钢圆管；&#xD;&#xA;4、承力脚：不锈钢可调式子弹脚；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="239" Qdbm="031004014016" Mc="花洒龙头" Xmtz="1、台式单孔的水龙头底座&#xD;&#xA;2、不锈钢双扣软管；&#xD;&#xA;3、18”(457 mm) 进水口软管。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="240" Qdbm="030412001025" Mc="紫外线消毒灯 40W" Xmtz="1、电源：220～230V/50Hz；&#xD;&#xA;2、灯管功率：（20W）×2支；&#xD;&#xA;3、灭蚊蝇范围：60～150平方米&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="241" Qdbm="ZB030101001123" Mc="四层格栅货架 1500*500*1600" Xmtz="1、优质304不锈钢板制作；&#xD;&#xA;2、层板：厚度1.2mm不锈钢板制作；&#xD;&#xA;3、加强筋：厚度1.2mm不锈钢板；&#xD;&#xA;4、立柱：厚度1.5mm不锈钢板制作；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.20" Mc="其他" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="242" Qdbm="ZB030101001124" Mc="反渗透净水系统" Xmtz="1、五级过滤+UV杀菌装置，纯净水水质通过权威检测；&#xD;&#xA;2、70%以上纯水回收率，废水率低于30%；&#xD;&#xA;3、大小活水循环：储水箱、净水管道活水循环；&#xD;&#xA;4、正反冲洗：滤芯滤料反冲洗功能，保证过滤能力，延长滤芯使用寿命；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="243" Qdbm="ZB030101001125" Mc="商用空气消毒净化机 600*500*1480" Xmtz="1、额定功率：2300W&#xD;&#xA;2、额定电压：220V/50Hz&#xD;&#xA;3、风量：1200m3/h&#xD;&#xA;4、全优质不锈钢外壳，耐腐蚀、抗氧化，坚固耐用；&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="套" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.21" Mc="排烟、送风" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="244" Qdbm="030702003001" Mc="不锈钢板通风管道" Xmtz="1、名称：排油烟风管&#xD;&#xA;2、材质、厚度：不锈钢板1.0mm&#xD;&#xA;3、规格、形状：矩形风管&#xD;&#xA;4、管件、法兰等附件等设计要求：法兰连接&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="450" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="245" Qdbm="WB030701004002" Mc="防爆通风机 25000风量m3/h" Xmtz="1、风量：25000m3/h&#xD;&#xA;2、电机功率：380V/7.5KW；&#xD;&#xA;3、含配套电机检查接线调试&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="246" Qdbm="WB030701004003" Mc="低噪音排气机组 15000风量m3/h" Xmtz="1、风量：15000m3/h&#xD;&#xA;2、电机功率：380V/3KW；&#xD;&#xA;3、转速：740r/min，全压：775Pa；&#xD;&#xA;4、含配套电机检查接线调试&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="247" Qdbm="WB030701004004" Mc="离心通风机 40000风量m3/h" Xmtz="1、风量：40000m3/h&#xD;&#xA;2、电机功率：380V/11KW；&#xD;&#xA;3、转速：770r/min，全压：775Pa；&#xD;&#xA;4、含配套电机检查接线调试&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="248" Qdbm="WB030701004005" Mc="离心通风机 30000风量m3/h" Xmtz="1、风量：30000m3/h&#xD;&#xA;2、电机功率：380V/11KW；&#xD;&#xA;3、转速：770r/min，全压：775Pa；&#xD;&#xA;4、含配套电机检查接线调试&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="249" Qdbm="WB030701004006" Mc="离心通风机 45000风量m3/h" Xmtz="1、风量：45000风量m3/h&#xD;&#xA;2、电机功率：380V/7.5KW；&#xD;&#xA;3、转速：770r/min，全压：775Pa；&#xD;&#xA;4、含配套电机检查接线调试&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="250" Qdbm="WB030701004007" Mc="离心通风机 20000风量m3/h" Xmtz="1、风量：20000风量m3/h&#xD;&#xA;2、电机功率：380V/18.5KW；&#xD;&#xA;3、转速：770r/min，全压：775Pa；&#xD;&#xA;4、含配套电机检查接线调试&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="251" Qdbm="030702003002" Mc="不锈钢板通风管道" Xmtz="1、名称：排油烟风管&#xD;&#xA;2、材质、厚度：不锈钢板1.0mm&#xD;&#xA;3、规格、形状：矩形风管&#xD;&#xA;4、管件、法兰等附件等设计要求：法兰连接&#xD;&#xA;5、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="1260" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="252" Qdbm="030703001001" Mc="防火阀 与烟管配套" Xmtz="1、280℃熔断自动关闭；该阀门安装在有防烟、防火要求的通风、空调系统的管道上，平时处于常开状态，火灾时关闭起到防烟阻火的作用；温控：温感器动作阀门自动关闭；电控：消防中心电信号（DC24V）电磁铁动作阀门自动关闭；手动关闭、手动复位；关闭后输出一组有源触点信号和一组无源触点信号&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、阀体安装&#xD;&#xA;2、支架制作、安装" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="253" Qdbm="030703007001" Mc="可调百叶鲜风口 300*300" Xmtz="1、型号：双层可调节&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="254" Qdbm="030404017006" Mc="风柜减震系统 配风柜" Xmtz="1、以金属弹簧为主，组合一定的阻尼材料；&#xD;&#xA;2、具有频率低，阻尼大、适用范围广，隔振降噪效果明显的功能；&#xD;&#xA;3、采用钢弹簧与橡胶串联形式组合隔振降噪元件。&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="1、采购、安装&#xD;&#xA;2、焊压接线端子&#xD;&#xA;3、接地" Jsgz="按设计图示数量计算" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="255" Qdbm="ZB030101001126" Mc="星三角启动保护器" Xmtz="1、具有缺相、过载、启动三重保护。&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="台" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="256" Qdbm="WB030701004008" Mc="油烟净化器 40000风量m3/h" Xmtz="1、外壳采用1.2mm以上厚度的碳钢，热固性纯聚酯粉末涂料喷涂工艺 抗紫外线耐候性好，设备提升防潮防晒性能，防溅、抗水、防尘，设备更适合户外使用，寿命更长&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="257" Qdbm="WB030701004009" Mc="油烟净化器 30000风量m3/h" Xmtz="1、设备净化效率不少于 98%。&#xD;&#xA;2、电源为智能数字电频高压电源。 &#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="258" Qdbm="WB030701004010" Mc="油烟净化器 45000风量m3/h" Xmtz="1、设备净化效率不少于 98%。&#xD;&#xA;2、电源为智能数字电频高压电源。 &#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="259" Qdbm="WB030701004011" Mc="油烟净化器 20000风量m3/h" Xmtz="1、设备净化效率不少于 98%。&#xD;&#xA;2、电源为智能数字电频高压电源。 &#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="260" Qdbm="WB030701005001" Mc="设备支架制作安装" Xmtz="1、名称：型钢支架&#xD;&#xA;2、规格：按要求自行制作&#xD;&#xA;3、风机、风阀、消声器、静压箱等支架&#xD;&#xA;4、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示质量计算" Dw="kg" Sl="1100" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="261" Qdbm="031201003001" Mc="金属结构刷油" Xmtz="1、油漆品种：除锈后均涂樟丹防锈漆两道&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="7940" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="262" Qdbm="031301012001" Mc="工程系统检测、检验" Xmtz="1、暖通系统调试费&#xD;&#xA;2、具体详见图纸、图集、技术规格书、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="263" Qdbm="031301017001" Mc="脚手架搭拆" Xmtz="1、脚手架搭拆费&#xD;&#xA;2、具体详见图纸、图集、技术规格书、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="AC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="AC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="AC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.7" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="AC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.3" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="AC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.6" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="AC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="AC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="AC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="8" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="140000" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje>
    <ZljeMx Xh="1" Mc="暂列金" Dw="" Zdje="140000" Bz="" />
  </Zlje>
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
  </Dxgcxx>
</JingJiBiao>