<?xml version="1.0" encoding="utf-8"?>
<JingJiBiao Xmbh="xm001" Xmmc="淮南高新区三和镇徐洼村村部道路工程" Version="1.0" Jsfs="一般计税" Jsdw="淮南市三和镇人民政府" Zjzmj="0">
  <ZhaoBiaoXx Zbr="淮南市三和镇人民政府" Zxr="安徽诚大建设项目管理有限公司" ZbrDb="张祝标" ZxrDb="倪龙松" Bzr="胡影" Fhr="朱明班" BzRq="2022-05-26" FhRq="2022-05-26" />
  <Dxgcxx Dxgcmc="淮南高新区三和镇徐洼村村部道路工程" Dxgcbh="dx001" Je="0" Bkjzf="0" Aqwmf="0" Zgj="0" Jzmj="0">
    <Dwgcxx Dwgcbh="00001" Dwgcmc="淮南高新区三和镇徐洼村村部道路工程" Zylb="4" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D83345C1ADCE5C67D11E5A64D564D428860A95DCE14113946CDB377BA186604042838BF9911442890" DogNum="9761220000004094" MachineKey="74-27-EA-A2-3B-51">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="SF-01" Mc="    环境保护费" Qfjs="0" Fl="3.57" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="SF-02" Mc="    文明施工费" Qfjs="0" Fl="7.33" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="SF-03" Mc="    安全施工费" Qfjs="0" Fl="5.28" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="SF-04" Mc="    临时设施费" Qfjs="0" Fl="7.99" Je="0" Fyxlb="1.4" />
  </Bkjzf>
  <Sj>
    <SjMx Xh="1" Mc="税金" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费-暂列金额" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="一" Mc="袁庄养老院至银杏苑一号安置点路口" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="040101005001" Mc="挖淤泥、流砂" Xmtz="1、沟塘处理清淤&#xD;&#xA;2、挖掘深度：1.5米&#xD;&#xA;3、运距：投标单位自行考虑&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示位置、界限以体积计算" Dw="m3" Sl="332" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="040103001001" Mc="回填方" Xmtz="1、清表回填处理&#xD;&#xA;2、填方材料要求：4%石灰土&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="332" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="040103001002" Mc="回填方" Xmtz="1、回填处理&#xD;&#xA;2、填方材料要求：50cm碎石&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="111" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="041001001001" Mc="拆除路面" Xmtz="1、拆除原砼道路结构&#xD;&#xA;2、材质：C30混凝土24cm&#xD;&#xA;3、碎石基层15cm&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按拆除部位以面积计算" Dw="m2" Sl="5850" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="5" Qdbm="041001001002" Mc="拆除路面" Xmtz="1、拆除地坪结构&#xD;&#xA;2、材质：C25混凝土15cm&#xD;&#xA;3、碎石基层10cm&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按拆除部位以面积计算" Dw="m2" Sl="2800" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="WB011614004001" Mc="建筑垃圾外运" Xmtz="1、建筑垃圾外运&#xD;&#xA;2、建筑垃圾种类：拆除的混凝土面层及碎石基层&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按需外运的建筑垃圾，以体积计算" Dw="m3" Sl="2870.5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="041001010001" Mc="路灯移位" Xmtz="1、现状路灯移位&#xD;&#xA;2、含基础&#xD;&#xA;3、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="按拆除部位以数量计算" Dw="盏" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="040203006001" Mc="沥青混凝土" Xmtz="1、沥青混凝土种类：AC-13C 细粒式改性沥青混凝土 SBS(Ⅰ-C)（掺 0.5%抗车辙剂）&#xD;&#xA;2、厚度：5cm&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="7350" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="040203004001" Mc="封层" Xmtz="1、下封层&#xD;&#xA;2、材料品种： ES-2 型矿料级配 BC-1 型乳化沥青稀浆封层&#xD;&#xA;3、厚度为 1cm&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="7350" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="040203003001" Mc="透层" Xmtz="1、材料品种：乳化沥青（PC-2）透层油&#xD;&#xA;2、喷油量： 0.7~1.5L/m2 &#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="7350" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="040202015001" Mc="水泥稳定碎（砾）石" Xmtz="1、水泥含量： 5％水泥稳定碎石&#xD;&#xA;2、厚度：30cm 厚&#xD;&#xA;3、压实度≥98％(15cm+15cm，层间洒水泥净浆)&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="8350" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="040202002001" Mc="石灰稳定土" Xmtz="1、含灰量：10％石灰土&#xD;&#xA;2、厚度：20cm &#xD;&#xA;3、压实度≥97％&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="8670" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="040201004001" Mc="路床石灰土改良土" Xmtz="1、路床 20cm 厚 6％石灰土改良土 93％&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="1734" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="040204004001" Mc="安砌混凝土侧石" Xmtz="1、道路侧石&#xD;&#xA;2、材料品种、规格： 水泥混凝土材质75X15X10cm&#xD;&#xA;3、抗压强度均要求不小于 30MPa&#xD;&#xA;4、2cm1:3水泥砂浆砌筑&#xD;&#xA;5、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示中心线长度计算" Dw="m" Sl="3330" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="WB040204011001" Mc="侧缘石垫层" Xmtz="1、侧石基础&#xD;&#xA;2、材料品种：C20砼&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="100" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="040101001001" Mc="挖一般土方" Xmtz="1、清除地表挖方&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="3000" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="040205002001" Mc="电缆保护管" Xmtz="1、现状管线保护&#xD;&#xA;2、工程量暂定，按实结算&#xD;&#xA;3、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="" Dw="m" Sl="200" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="18" Qdbm="040504001001" Mc="砌筑检查井" Xmtz="1、现状检查井维修改造&#xD;&#xA;2、工程量暂定，按实结算&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="040205019001" Mc="减速垄" Xmtz="1、材料品种：橡胶减速带&#xD;&#xA;2、规格、型号：橡胶材质、规格为38×50×5cm&#xD;&#xA;3、端节、端头按黄色、黑色相间设置，与沥青路面间用橡胶螺栓固定&#xD;&#xA;4、反光珠为Φ10白色透亮材质&#xD;&#xA;5、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="" Dw="m" Sl="24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="040205003001" Mc="立杆式交通标志（单牌）" Xmtz="1、类型：交通标牌&#xD;&#xA;2、包含面板、杆件、基础&#xD;&#xA;3、未尽事宜详见图纸、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="040205018001" Mc="警示桩" Xmtz="1、材料品种：路口警示桩&#xD;&#xA;2、8个路口&#xD;&#xA;3、路口警示桩采用120*3钢管，在管内填入C30混凝土，柱身红、白反光涂料。&#xD;&#xA;4、C30砼基础400*400*400&#xD;&#xA;5、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="040101005002" Mc="挖淤泥、流砂" Xmtz="1、现状沟清淤疏通&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="" Dw="m" Sl="1000" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="ZB040203015001" Mc="新旧路面搭接" Xmtz="1、新旧路面搭接&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="" Dw="处" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="WB041101015001" Mc="彩钢板施工围栏搭拆" Xmtz="1、材料品种：施工围栏&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示以长度计算" Dw="m" Sl="34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="040205006001" Mc="标线" Xmtz="1、材料品种：白色热熔标线&#xD;&#xA;2、热熔型反光涂料&#xD;&#xA;3、标线涂层厚度1.8mm±0.2mm&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="520" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="二" Mc="陶东组徐作贤家至陶永刚家" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="26" Qdbm="041001001003" Mc="拆除路面" Xmtz="1、拆除原砼道路结构&#xD;&#xA;2、材质：C30混凝土&#xD;&#xA;3、厚度：20cm&#xD;&#xA;4、工程量暂定，按实结算" Gcnr="" Jsgz="按拆除部位以面积计算" Dw="m2" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="041001007001" Mc="拆除砖石结构" Xmtz="1、结构形式：拆除砖砌构筑物" Gcnr="" Jsgz="按拆除部位以体积计算" Dw="m2" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="WB011614004002" Mc="建筑垃圾外运" Xmtz="1、建筑垃圾外运&#xD;&#xA;2、建筑垃圾种类：拆除的混凝土面层及碎石基层&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按需外运的建筑垃圾，以体积计算" Dw="m3" Sl="4.4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="29" Qdbm="040202001001" Mc="路床(槽)碾压检验" Xmtz="1、路床(槽)碾压检验&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计道路底基层图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="445" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="040202011001" Mc="级配碎石" Xmtz="1、厚度：8cm厚级配碎石基层&#xD;&#xA;2、原泥石路夯实，压实度≥92%&#xD;&#xA;3、未尽事宜详见图纸、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="445" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="040203007001" Mc="水泥混凝土" Xmtz="1、新建水泥砼路面&#xD;&#xA;2、混凝土强度等级：C30水泥混凝土面层（弯拉强度≥4.0MPa）&#xD;&#xA;3、厚度：15cm&#xD;&#xA;4、伸缩缝及传力杆&#xD;&#xA;5、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="445" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="32" Qdbm="040501004001" Mc="塑料管铺设" Xmtz="1、管道材质：D200过路管&#xD;&#xA;2、管径：200&#xD;&#xA;3、包含安装所需支架附件等&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="040504001002" Mc="砌筑检查井" Xmtz="1、砖砌方井500*500&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="040205018002" Mc="警示桩" Xmtz="1、材料品种：路口警示桩&#xD;&#xA;2、路口警示桩采用120*3钢管，在管内填入C30混凝土，柱身红、白反光涂料。&#xD;&#xA;3、C30砼基础400*400*400&#xD;&#xA;4、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="040101001002" Mc="挖一般土方" Xmtz="1、清除地表挖方&#xD;&#xA;2、余方弃置&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="120" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="040103001003" Mc="回填方" Xmtz="1、清表回填处理&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="三" Mc="西北组徐基月家至徐之刚家" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="37" Qdbm="041001007002" Mc="拆除砖石结构" Xmtz="1、结构形式：拆除砖砌构筑物&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按拆除部位以体积计算" Dw="m2" Sl="18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="38" Qdbm="WB011614004003" Mc="建筑垃圾外运" Xmtz="1、建筑垃圾外运&#xD;&#xA;2、建筑垃圾种类：拆除的混凝土面层及碎石基层&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按需外运的建筑垃圾，以体积计算" Dw="m3" Sl="4.32" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="050102001001" Mc="栽植乔木" Xmtz="1、树木移植&#xD;&#xA;2、胸径：18cm&#xD;&#xA;3、就近移植，常规养护&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示数量计算" Dw="棵" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="041001010002" Mc="路灯移位" Xmtz="1、现状路灯移位&#xD;&#xA;2、含基础&#xD;&#xA;3、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="按拆除部位以数量计算" Dw="盏" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="040202001002" Mc="路床(槽)碾压检验" Xmtz="1、路床(槽)碾压检验&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计道路底基层图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="975" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="040202011002" Mc="级配碎石" Xmtz="1、厚度：8cm厚级配碎石基层&#xD;&#xA;2、原泥石路夯实，压实度≥92%&#xD;&#xA;3、未尽事宜详见图纸、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="975" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="040203007002" Mc="水泥混凝土" Xmtz="1、新建水泥砼路面&#xD;&#xA;2、混凝土强度等级：C30水泥混凝土面层（弯拉强度≥4.0MPa）&#xD;&#xA;3、厚度：15cm&#xD;&#xA;4、伸缩缝及传力杆&#xD;&#xA;5、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="975" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="44" Qdbm="040501004002" Mc="塑料管铺设" Xmtz="1、管道材质：D200 过路管&#xD;&#xA;2、管径：200&#xD;&#xA;3、包含安装所需支架附件等&#xD;&#xA;4、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="040504001003" Mc="砌筑检查井" Xmtz="1、砖砌方井500*500&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="46" Qdbm="040205018003" Mc="警示桩" Xmtz="1、材料品种：路口警示桩&#xD;&#xA;2、路口警示桩采用120*3钢管，在管内填入C30混凝土，柱身红、白反光涂料。&#xD;&#xA;3、C30砼基础400*400*400&#xD;&#xA;4、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="040101001003" Mc="挖一般土方" Xmtz="1、清除地表挖方&#xD;&#xA;2、余方弃置&#xD;&#xA;3、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="240" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="040103001004" Mc="回填方" Xmtz="1、清表回填处理&#xD;&#xA;2、未尽事宜详见图纸、说明书、答疑、招标文件及相关规范" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="041106" Mc="大型机械设备进出场及安拆" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="49" Qdbm="041106001001" Mc="大型机械设备进出场及安拆" Xmtz="1、大型机械设备进出场及安拆&#xD;&#xA;2、其他未尽事宜详见招标文件、图纸会审、答疑、设计图纸及满足相关规范要求" Gcnr="" Jsgz="按使用机械设备的数量计算" Dw="台·次" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="SC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="SC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1.2" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="SC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="SC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="SC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.9" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="SC-06" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="7" Xmbm="SC-07" Mc="行车、行人干扰增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="9" />
      <ZjCsMx Xh="8" Xmbm="SC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="8" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="140000" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
    <QtxmMx Xh="5" Mc=" " Dw="" Je="0" Bz="" Xmlb="0" />
  </Qtxm>
  <Zlje>
    <ZljeMx Xh="1" Mc="暂列金额" Dw="" Zdje="140000" Bz="" />
  </Zlje>
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
  </Dxgcxx>
</JingJiBiao>